# Question#01

Administrative Distance: 120 (RIP)

# Question#02

Administrative Distance: 110 (OSPF)

# Question#03

Administrative Distance: 1 (Static)

# Question#04

Static Routing is used when we have a small network/topology like a home network. Dynamic Routing is used when we have large and complex network/topologies.